#### Parameters Setup

Selecting wRs Parms, write in the RF Ch window the radio channel number (1 .. 267) and press Program: the old parameter is erased (E) and in sequence the new value is written (W).
When the operation is completed it will appear 'W 100%'. In case of problems, repeat the operation.
Select wEc/wTn Parms in order to setup Sensors parameters.
The wEc and wTn devices must be programmed one at a time and for this reason, it is suggested to switch off all of them, in case they are on, by pressing their On/Off buttons and proceed as follows:
1) Keep pressed the On/Off button of the first device which one intends to program until the Sensor Led will switch on (about 3 sec).
2) Click on Select in order to switch between Sensor 1 (S1 - red trace) and Sensor 2 (S2 - blue trace). Keep in mind that the wEc unit cannot be programmed as Sensor 2.
3) Click on Program.
The radio channel will be programmed according to the wRs one.
The old parameter is erased (E) and in sequence, the new value is written (W).
When the operation is completed it will appear 'W 100%'. In case of problems, repeat the operation.
If the unit does not respond, remove and reinsert the battery.
Check in the Status Panel that the operation was successful, otherwise repeat the procedure.
Switch off the programmed unit ((On/Off button for about 3 sec) and repeat the steps from 1 to 3 with the other sensors.
Once the devices have been programmed, exit the 'Device programming' mode by disabling the 'Enable Prog. Mode' button.