#### Ecg + Tonometer / Two Tonometers

The Software automatically recognizes the connection of the Ecg module + Tonometer or two Tonometers.
Ecg + Tonometer
The Ecg module is always set as Sensor 1 - red trace (single beep during power on).
The Tonometer must be set as Sensor 2 - blue trace (double beep during power on).
Two Tonometers
First Tonometer must be set as Sensor 1 - red trace (single beep during power on).
The second Tonometer must be set as Sensor 2 - blue trace (double beep during power on).
Wrong Configurations
In this case, the Tonometer is set as Sensor 1 (single beep during power on) and conflicts with the Ecg module that is always Sensor 1 - red trace (single beep during power on).
Other wrong situations are two Tonometers both of them as Sensor 1 or Sensor 2.
Factory settings are as follows:
WPP001-ET: Tonometer with black o-ring settled as Sensor 2
WPP001-ETT: Tonometer with red o-ring settled as Sensor 1 and Tonometer with black o-ring settled as Sensor 2
Please refer to the ' Parameter Setup ' paragraph in order to switch between mode Tonometer Sensor 1 and Tonometer Sensor 2.