#### Status Panel

The status panel includes one row for each unit, from the top to the bottom:
wRs (USB unit)
wEc (ECG unit) / wTn (Tonometric unit) : Sensor 1 - red trace
wTn (Tonometric unit) : Sensor 2 - blue trace
The columns contain the following information:
App. Fw: version of the application Firmware loaded on the device
RF Ch: radio channel
Boot Loader: version of the startup Firmware (cannot be modified by the user)
MS/n: serial number of the wRs unit linked to the device
S/n: serial number of the unit
Hw Rel.: hardware release
Calib: calibration parameter
By clicking on the diskette icon on the right you can save to file the contents of the status panel.