#### ECG

To remove an ECG complex from the signal analysis, place the mouse pointer on the blue dot corresponding to the R wave peak and click with the left mouse button.
A blue vertical line appears: the ECG complex has been selected.
Select the icon on the right of the monitor to delete the ECG complex.
The disappearance of the blue dot confirms the deletion of the ECG complex from the signal analysis.
Only when the number of ECG complex is less than 10 it's possible to insert a new one.
To insert a new ECG complex select the icon on the right of the monitor, therefore place the mouse pointer on the R wave peak.
Click with the left mouse button: the appearance of the blue dot confirms the insertion of the ECG complex.
Now you can select and move the blue line to improve the position of the marker.
Select the below icon to close the recording analysis and return to see the whole recording.
Finally, confirm the changes.